### Conduit & Piping Layout

First-fix structural preparation, uncoiling heavy-duty flexible protective conduits for secure refrigerant and drainage line routing.

### Multi-Unit VRF Rough-In

Suspended ceiling installation of indoor chassis units wrapped for protection, integrated with premium insulated copper pipe networks.

### Custom Joinery HVAC Integration

Sleek, minimalist linear supply grilles integrated seamlessly above premium bespoke wardrobe units in a high-end interior development.

### Drop-Ceiling Bulkhead Diffusers

Completed ceiling bulkhead configuration featuring dual linear slot diffusers paired with elegant architectural cove lighting.

### Central Ducted Infrastructure

Precision fabrication and routing of pre-insulated, high-velocity air distribution networks along raw structural slabs.

### VRV System Commissioning

Installation of high-efficiency Daikin VRV X inverter outdoor condenser arrays for multi-zone climate control.

No projects in this category yet.

## Three problems, and exactly how we solved them.

### Alpha Praxis Headquarters & Commercial Complex

##### The Context

As a multi-tenant commercial complex, the facility required a high-capacity climate solution capable of handling variable thermal loads across different office layouts without driving up energy overheads.

##### Engineering Solution

We engineered and executed the precision piping and installation of a Variable Refrigerant Volume (VRV) ceiling cassette system. This setup allows localized temperature control for individual zones, ensuring optimized airflow mapping across the entire corporate infrastructure.

##### The Outcome

Delivered an energy-efficient, whisper-quiet cooling matrix that adapts dynamically to building occupancy, resulting in lower operational costs and maximum tenant comfort.

### Executive Private Residence

##### The Context

The architectural brief for this premium estate demanded a powerful, multi-room cooling system that would completely preserve the sophisticated interior aesthetics and high ceilings of the home.

##### Engineering Solution

Supplied and installed premium split ceiling-concealed units. By housing the bulk of the mechanical hardware within the ceiling voids, we delivered seamless climate control accessible only via minimalist linear diffusers that blend directly into the drywall architecture.

##### The Outcome

Achieved a pristine, uncompromised interior design profile with multi-zone cooling control, offering personalized luxury comfort room by room.

### Judges Quarters (Yellow House)

##### The Context

This high-profile institutional residence required a comprehensive, centralized cooling overhaul that balanced heavy-duty structural durability with quiet, dignified living spaces.

##### Engineering Solution

We deployed a comprehensive VRV Ceiling-Concealed Ducted System. This architecture utilizes hidden duct networks to distribute balanced, conditioned air uniformly across massive floor plates, managed by centralized smart thermostats.

##### The Outcome

Eliminated hotspots entirely across the property while maintaining an ultra-low acoustic footprint, proving that massive cooling power can be completely silent.

### Bonzi Complex

##### The Context

Located in a high-traffic commercial zone, this venue experiences rapid spikes in foot traffic and high ambient heat-loads, demanding an aggressive, industrial-grade cooling response.

##### Engineering Solution

We supplied and commissioned heavy-duty, Large Ducted Central Systems. The layout was calculated to maximize volume air changes per hour, driving massive quantities of cooled air through engineered high-velocity duct networks designed for dense commercial spaces.

##### The Outcome

Rapid thermal recovery times—the system can cool down high-occupancy spaces within minutes of full activation, even during peak afternoon exterior temperatures.

### The Oasis Auditorium

##### The Context

Large worship auditoriums present unique HVAC challenges: massive open vertical spaces, expansive ceiling heights, and sudden, extreme weekend occupancy loads.

##### Engineering Solution

We designed a hybrid cooling strategy, supplying and installing a high-capacity mix of Floor-Standing and Ceiling Cassette Units. The cassettes provide widespread down-draft cooling from above, while the standing units offer immediate, high-volume perimeter air displacement right at the crowd level.

##### The Outcome

Achieved perfect thermal equilibrium throughout the vast hall, ensuring a comfortable environment for worshippers from the front rows all the way to the back gallery.

## Have a project that needs this level of precision?

Book a site assessment and we'll approach yours the same way.

## Book a Site Assessment

Pick a date and share your project details — our engineering team will confirm within one business day.

1Select date & time
Su Mo Tu We Th Fr Sa
Available times

Select a date to see available times.

2Project details
Full name *
Phone number *
Project type
Preferred system
Scope / description

No date selected yet.

No commitment for the initial assessment.

Chat on WhatsApp